**UPDATING FIRMWARE ON THE TTM430, TTM430SC and TTM460**

1. Make sure your printer is powered off.
2. Click this link [Printers | HellermannTyton](https://www.hellermanntyton.us/support/id-solutions/printers) Scroll down to ***“Firmware Update”***, select ***“TTM430”*** Once you select the Firmware it should be downloaded
3. Click the file in the downloads drag it or copy to a USB stick in a directory named misc
4. Turn on printer.
5. Plug the USB stick into an open USB port in the back of the printer
6. Using the touch screen menu on the front of the printer, tap ***Settings*** icons, the ***Extras*** icon. Select the ***Firmware Update***.
7. ***USB Memory*** should already be highlighted in yellow. You should see the firmware file stored on the USB stick
8. Tap the ***green check mark*** at the bottom of the screen.
9. You will see a progress bar as the file loads. When complete, the printer will automatically restart
10. To see if the firmware update was successful, tap the ***Settings*** icon and then the ***Info*** icon to display the revision.